Manageability Mode = 0
Manageability Mode Lock = 0
Local Firmware Update Enabled = 0
Local FWU Override Counter = 0
Local FWU Override Qualifier = 1
Flash Descriptor Override Pin-Strap Ignore = 0
AMT Compatibility Mode = 0
AMT Configuration Mode = 0
ZTC Enable = 0
Configuration Server Port = 0
Configuration Server Name = ProvisionServer
Configuration Server IP = 0.0.0.0
AMT Host Name = IntelAMT
AMT Domain Name = intel.com
DHCP Enabled = 1
AMT Ping Response Enabled = 1
AMT Static IP Address = 10.0.0.2
AMT Static IP Subnet Mask = 255.255.255.0
AMT Static IP Default Gateway Address = 0.0.0.0
AMT Static IP Primary DNS Address = 0.0.0.0
AMT Static IP Secondary DNS Address = 0.0.0.0
AMT Dedicated MAC Address = 00-11-22-33-44-55
VLAN = 0
PET Language Code = 0x00
PET OEM Custom Fields 00-15 = 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
PET OEM Custom Fields 16-31 = 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
PET OEM Custom Fields 32-47 = 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
PET OEM Custom Fields 48-63 = 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
PET OEM Custom Fields Length = 0
PET Community String = public
AMTManuf Test Counter = 8
IDER Boot Capable = 1
SOL Boot Capable = 1
BIOS Reflash Capable = 0
Boot into BIOS Setup Capable = 0
Pause during BIOS Boot Capable = 0
HostIf SOL Enabled = 0
HostIf IDER Enabled = 1
Remote Wake Timer = 1
ME Visual LED Indicator Enabled = 1
LAN Power Well = 2
WLAN Power Well = 2
Power Package 1 Supported (Mobile: ON in S0) = 1
Power Package 2 Supported (Mobile: ON in S0, S3/AC) = 1
Power Package 3 Supported (Mobile: ON in S0, S3/AC, S4-5/AC) = 1
Power Package 4 Supported (Mobile: ON in S0; ME WoL in S3/AC) = 1
Power Package 5 Supported (Mobile: ON in S0; ME WoL in S3/AC, S4-5/AC) = 1
Default Power Package = 1
Kedron Driver WA = 1
AMT Legacy Provisioning Mode Supported = 1
AMT VLAN Local Configuration Blocked = 0
iQST Supported = 0
ASF Supported = 1
AMT Supported = 1
PKI DNS Suffix = amt.intel.com
