+============================================================================+
				ICL50/KAL10 ROM Release Note
+============================================================================+
BIOS CORE Version ................  Insyde EFI 2.0
CPUs Supported    ................  Intel Merom,Merom-Lite
Chipset           ................  Intel Crestline
Bridge            ................  Intel ICH8M
CardReader        ................  RICOH833,N/A(KAL10)
Video             ................  ATI M71M,M76M,N-vida NB8M,NB8M-SE,NB8M-GS,NB8P-GS,Intel
Audio             ................  Realtek ALC268 codec.
LAN               ................  Broadcom 5787KMLG(Nettiling),5906(Acadia 2/KAL10)
1394 controller   ................  RICOH833(Nettiling),N/A(KAL10)
KBC               ................  ENE926
Clock Generator   ................  ICS9LPRS365
Super I/O         ................  NONE
BIOS ROM Part	  ................  MX25LV008BB
+==============================================================================+
| MODEL NO. :  ICL50/KAL10                         RELEASE DATE : 07/23/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.44 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.44 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 46DA(FD)                                              |
+==============================================================================+
BIOS:
   None.

EC:
   1). Fix Media Activity LED always on issue.(KAL10)

+==============================================================================+
| MODEL NO. :  ICL50/KAL10                         RELEASE DATE : 06/25/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.43 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.43 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : BE67(FD)                                              |
+==============================================================================+
BIOS:
   1). Modify CL value to cover Micron RAM issue.
   2). Disable LAN ASPM and enable break event on AC mode.

EC:
   None.

+==============================================================================+
| MODEL NO. :  ICL50/KAL10                         RELEASE DATE : 06/11/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.42 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.42 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 5E44(FD)                                              |
+==============================================================================+
BIOS:
   1). Modify Dts function.
   2). Fix BSOD 77/7A.

EC:
   1). Workaround for Windows bar hangup issue.

+==============================================================================+
| MODEL NO. :  ICL50/KAL10                         RELEASE DATE : 05/20/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.41 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.41 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 090D(FD)                                              |
+==============================================================================+
BIOS:
   None.

EC:
   1). Add "Protect SPI ROM" function.

+==============================================================================+
| MODEL NO. :  ICL50/KAL10                         RELEASE DATE : 05/20/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.40 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.40 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 738F(FD)                                              |
+==============================================================================+
BIOS:
   1). Remove ATI M82M/M86M ASPM support on AC mode.
   2). Fix when resume from S4, system still display F2/F10 string.(For Rhine platform)
   3). Fix input password Not Case Sensitive on password dialog

EC:
   1). Chagne VGA thermal address from Local to Remote.
   2). Add work around for Linpus brightness problem.

+==============================================================================+
| MODEL NO. :  ICL50/KAL10                         RELEASE DATE : 05/15/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.39 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.39 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 3476(FD)                                              |
+==============================================================================+
BIOS:
   1). Fixed hang on windows bar.
   2). Fix battery can't charge after winflash.
   3). Set SMBIOS Type 0 BIOS Version is "EMACHINES" , not "Gateway"
   4). Change HDPSW Status to "Froze" and disable "Set HD Password" function after HDD Frozen.
   5). Fix when set the first password, then press shift + number key as second password, it will occur many lines of spaces.
   6). Fix Disable D2D in BIOS Setup, still can execute D2D.

EC:
    None.

+==============================================================================+
| MODEL NO. :  ICL50/KAL10                         RELEASE DATE : 05/07/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.38 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.38 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : C9BF(FD)                                              |
+==============================================================================+
BIOS:
   1). Add SVID of ATI M86M audio.

EC:
   1). Fix Media Activity LED always on issue.

+==============================================================================+
| MODEL NO. :  ICL50/KAL10                         RELEASE DATE : 05/06/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.37 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.37 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 52C1(FD)                                              |
+==============================================================================+
BIOS:
   1). Remove MIR on Rhine platform for S4 resume black screen.

EC:
   1.) Enable volume control by Fn + ¡ô¡B¡õ when Board ID 6.

+==============================================================================+
| MODEL NO. :  ICL50/KAL10                         RELEASE DATE : 05/05/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.36 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.36 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 9A6C(FD)                                              |
+==============================================================================+
BIOS:
    1). Combine ICL50/ICK70/KAL10
    2). Add KAL10 SVID
    3). Add KAL10 Post Logo
    4). Press F10 into Boot Menu (for KAL10)

EC:
   1). Add volume control by Fn + ¡ô¡B¡õ.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 04/29/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.35 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.35 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : FCB6(FD)                                              |
+==============================================================================+
BIOS:
   None

EC:
   1). Modify to new thermal control table V14 (Discrete system).
   2). Add M82M/M86M VGA thermal sensor reading function.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 03/26/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.34 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.34 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : BF3E(FD)                                              |
+==============================================================================+
BIOS:
   1). Enable Execute Disable Bit.
   2). Add ATI M86 VGA board.
   3). Fix BSOD 0x101.(update DTS function)
   4). Enable SATA port 2.
EC:
  1). None.
  
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 03/15/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.33 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.32 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 4956(FD)                                              |
+==============================================================================+
BIOS:
  1). Fixed BOBO sound when play music.
  2). Fixed can't via int15 function to get serial number
  3). Fixed Asset Tag issue.

EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 03/13/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.32 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.32 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 8647(FD)                                              |
+==============================================================================+
BIOS:
  1). Solve BOBO sound when play music.
  2). Implement ATI M82 VGA.

EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 03/10/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.31 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.31 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 8394(FD)                                              |
+==============================================================================+
BIOS:
  1). Improve BOBO sound when play music.

EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 03/03/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.30 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.30 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 3654(FD)                                              |
+==============================================================================+
BIOS:
  1). Implement SATA LPM workaround.
  2). Update MRC V1.04.
  3). Support new nVidia VGA. (NB8P-SE, NB9P-GE1, NB9M-GE1, NB9M-GS, NB9P-GE2, NB9M-GE)

EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 01/31/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.29 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.29 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 5D2B(FD)                                              |
+==============================================================================+
BIOS:
  1). Update Tj85 cpu fan-table for Thermal request.
  
EC: 
  1). Update new Thermal Control Table.
  
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 01/18/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.28 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.28 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 5B4B(FD)                                              |
+==============================================================================+
BIOS:
  1). Fix Pci Express LAN card can't used.

EC:
  1). Add Linux Flag for brightness hotkey with no SCI under linux OS.
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 01/05/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.27 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.27 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : A25F(FD)                                              |
+==============================================================================+
BIOS:
  1). When run camera AP, camera image will lag.
  
EC:
  None. 
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 01/02/2008   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.26 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.26 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.28                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 012B(FD)                                              |
+==============================================================================+
BIOS:
  1). update Chipset code.
  2). Support engineer sample Merom CPU CPUID:06FB
  3). Update Micro code CPUID: 6FD version ID: A3.
  4). Update Panel ID Table.
EC:
  1). Add new panel list follow 
      15" = "ICL50 BrightnessContorlTableV1.2"
      17" = "Acer_17inch_BrightnessControlTableV1.1"
  2). Add work around for S4 RTC wake issue.
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 12/23/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.25 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.25 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 2720(FD)                                              |
+==============================================================================+
BIOS:
  1). Update new solution for Penryn CPU.(Processor May Unexpectedly Assert False THERMTRIP# After
      Receiving a Warm Reset)
  
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 12/21/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.24 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.24 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 2653(FD)                                              |
+==============================================================================+
BIOS:
  1). Implement workaround for Penryn CPU. (Processor May Unexpectedly Assert False THERMTRIP# After
      Receiving a Warm Reset)
EC:
  1). Fix restore throtting function is not correct.
  2). Block Control+B or S key under APM mode to avoid Broadcom issue.
  3). Remove brightness SCI event to avoid brightness control problem
      under Linux.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 12/17/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.23 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.23 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 74CC(FD)                                              |
+==============================================================================+
BIOS:
  1). Fixed DTM can't pass for Penryn CPU.
  2). Fix "Add Asset Tag" button disappear issue.

EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 12/12/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.22 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.22 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1518                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 5A3C(FD)                                              |
+==============================================================================+
BIOS:
  1). Modify OS shutdown temperature from 100 to 110.
  2). Modify nVidia VGA string offset.
  3). Fixed S3 resume will shutdown on CM530 platform.

EC:
  1). Add TJ85 DTS 85 degC shutdown function.
  2). Update Fan table V12.
      Under Penryn CPU, Fan will only refer to T-Diode temperature.
  3). Add Command for Penryn CPU. Cmd45 Dat29
  4). Add "write 0x15 to thermal sensor" function to support 
      Penryn CPU thermal sensor.
  5). Modify 6 Cell define criteria to support 6 cell battery has 
      different design capacity.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 11/08/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.21 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.21 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 0376(FD)                                              |
+==============================================================================+
BIOS:
  1). Add Penryn CPU support.
  2). Fixed POST time too long if setup memory over 2G.
  3). Implement workaround for BroadCom W-lan Disable L0,L1s.

EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 11/01/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.20 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.20 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 719A(FD)                                              |
+==============================================================================+
BIOS:
  1). None.

EC:
  1). Modify T-Diode throtting temp from 100 to 95 degC

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 10/15/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.19 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.19 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 3C36(FD)                                              |
+==============================================================================+
BIOS:
  1). Modify Verbtable.
  
EC:
  1). Modify TouchPad packet timeout timer for system with ALPS touchpad
 	    & KB typing delay issue.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 09/26/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.18 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.18 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 9FD0(FD)                                              |
+==============================================================================+
BIOS:
  1). Implement workaround for nVidia VGA and enable L1 ASPM.
  2). Verify VBIOS string number address.
  
EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 09/14/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.17 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.17 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : F194(FD)                                              |
+==============================================================================+

BIOS:

EC:
  1). Modify EC_TX/EC_RX control method to prevent Intel 4965 WL card
	    SSID lose issue.
	    
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 09/10/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.16 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.16 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 91FF(FD)                                              |
+==============================================================================+
BIOS:

  1). Fixed mouse disperser when install WinXP OS
  2). Fixed MIR & Mother resource collision issue
  3). Add 2 second delay for TOSHIBA HDD issue into reboot phase.
  4). Add a SSID for NVIDIA NB8P-GS.

EC:
  1). Modify SPI write/earse behavior to support correct MXIC & SST
	  write/earse behavior.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 09/03/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.15 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.15 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   : AE81H(FD)                                          |
+==============================================================================+
BIOS:
  1). Add new AUO(B154EW04 VB) panel and notify EC Panel ID.
  2). Update NB8P-GS Version and UUID String.

EC:
  1). Add new AUO Panel (B154EW04 VB) to brightness table.
  2). Modify Media LED control signal for Acadia system.
  3). Modify SPI write/earse function to support SST SPI ROM.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 08/09/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.14 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.14 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & Insyde WinFlash 3.23                      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   : C4B7H(FD)                                          |
+==============================================================================+
BIOS:
  1).Disable C4 function for T2330 and T2310.
  2).Implement Throttle function on DOS mode.
  3).Fixed ODD serial number error.
  4).Update Acadia 2 Verb Table.
	
EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 07/28/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.13 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.13 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & ENEFLASH.EXE 0.15& Insyde WinFlash 3.23   |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   : 89DEH(FD)                                          |
+==============================================================================+
BIOS:
	1). Fixed s3 resume will cause OS lag under 4G platform.
	2). Add New Microcode for T7700 and T7500.
	3). Implement Workaround for Two hdd swap issue.
	4). Implement SSID/SVID for ASKEY modem.
	
EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 07/19/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.12 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.12 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & ENEFLASH.EXE 0.15& Insyde WinFlash 3.23   |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   : 5A45H(FD)                                          |
+==============================================================================+
BIOS:
	1). If close panel and boot to Vista, Panel device can't be detect.
	2). Implement Memory support capability for 965/960 on DMI string.
	3). Modify DTS function.
	4). Add support ACPI3.0 and fixed BSOD 7E when system restore.
	
EC:
  1). Modify WL_OFF control sequence to fix WLAN SSID lose issue.	

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 07/12/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.11 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.11 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & ENEFLASH.EXE 0.15& Insyde WinFlash 3.17   |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   : E0F0(FD)                                           |
+==============================================================================+
BIOS:
	1). Fix BSOD under 4G platform.
	2). Update VGA BIOS Version of SystemInformation Menu.
	3). Fixed BSOD 0x7E issue.
	
EC:
  1). None.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 07/04/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.10 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.10 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & ENEFLASH.EXE 0.15& Insyde WinFlash 3.17   |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   : 2DD8(FD)                                           |
+==============================================================================+
BIOS:
	1). Add workaround for Turbo Memory.
	2). Append SSID Table for Acadia 960.
	3). Append HD Verb Table for Acadia 960.
	4). Added 17" LCD Panel Type to inform EC.
	5). Fixed could not show password message when use E-setting set password.
	6). Enable DTS function.
	
EC:
  1). Update Brightness table to support two more panel.
	    AUO and Samsung.
	2). Enable DTS function.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 06/28/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.09 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.09 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & ENEFLASH.EXE 0.15& Insyde WinFlash 3.17   |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   : F01C(FD)                                           |
+==============================================================================+
BIOS:
	1). Disable MIR Function of Acadia 960.
	2). Update BCM5906 LAN control for Acer EPM.
	3). Add SATA Mode Support AHCI/IDE control for Acer request.
	4). Dynamic to report SMBIOS Type 2, add Acadia 960 Platform.
	
EC:
  1). Modify Read Charing Voltage function to avoid SANYO battery
 	    will not be able to be charged when battery cycle count over
 	    100.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 06/21/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.08 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.08 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & ENEFLASH.EXE 0.15& Insyde WinFlash 3.17   |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   : 364C(FD)                                           |
+==============================================================================+
BIOS:
	1). Add support nVidia VGA at setup Menu.
	2). Add support SST 25VF080B flash part.
	3). Add support Chicony 0.3M CCD.
	4). Disable MIR and Brightness function at Windows XP.
	5). Fixed S3 resume black screen with CM540 CPU.
	6). Add support Robson card.
	7). Fixed [x64 eSetting 2.5.3003] Blue screen after eSettings n ETF.
	8). Fixed Linups function can't control SLP.
	
EC:

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 06/07/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.07 (for MP-EN)        CPU u-code Version:          |
|   KBC BIOS Version   : V1.07 (for MP-EN),                                    |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & ENEFLASH.EXE 0.15& Insyde WinFlash 3.17   |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   : B078(FD)                                           |
+==============================================================================+
BIOS:
	1). Fixed during flash process , Fan can't always on sometime.
	2). Added Broadcom PCIE 5906 LAN.
	3). Update Merom L CPU Micro Code.
	4). Fixed Two Hitachi HDDs can't resume form s3.
	5). Fixed Sometimes No-Video between flash done and reboot.
	
EC:
	1). Modify TJ85 CPU T-Diode shutdown temperature from 90 degC
 	    to 85 degC and TJ100 CPU from 105 to 100 degC.
  2). Modify flash behavior to avoid system hang after flash.
	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 05/22/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.06 (for UMA Golden)        CPU u-code Version:     |
|   KBC BIOS Version   : V1.06 (for C),                                        |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.2 & ENEFLASH.EXE 0.15& Insyde WinFlash 3.17   |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   :  DF70(FD)                                          |
+==============================================================================+
BIOS:
	1). Change flash procedures.(only use Idle command once while flashing).
	2). Solved USB Speaker noise when set power saver mode.
	3). Disable Remove function of TV tuner.

EC:
	1). Add Cmd for TJ85 CPU and Fan table for TJ85 CPU.
  2). Check System LED status during "turn off system"
 	    to aviod suspend led on after press power button for
 	    resuming from S4.
	3). Update Fan table to follow thermal control table v06.
	4). Modified Fan control function to identify fan table for
 	    UMA and Discrete system.
 	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 05/17/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.05 (for UMA Golden)        CPU u-code Version:     |
|   KBC BIOS Version   : V0.25 (for C),                                        |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.1R & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.05 (FD)   :  CBA9(FD)                                          |
+==============================================================================+
BIOS:
        1). Enable CPU Turbo mode let CPU change state smooth.
EC:
   REMOVE
 	1). Update Fan table to follow thermal control table v06.
 	2). Modified Fan control function to identify fan table for
 	    UMA and Discrete system.
 	3). Check System LED status during "turn off system"
 	    to aviod suspend led on after press power button for
 	    resuming from S4.
	4). Add Cmd for TJ85 CPU and Fan table for TJ85 CPU.
	    TJ85 fan table is follow Thermal Fan table V0.6
 	    Cmd 45 Dat 28. 	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 05/15/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.03 (for UMA Golden)        CPU u-code Version:     |
|   KBC BIOS Version   : V1.03 (for C),                                        |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.03 (FD)   :  1A4C(FD)                                          |
+==============================================================================+
BIOS:
        1). Implement Dummy HDD
	2). Fixed Audio noise.
	3). Remove DTS function
EC:
 	1). Update Fan table to follow thermal control table v06.
 	2). Modified Fan control function to identify fan table for
 	    UMA and Discrete system.
 	3). Check System LED status during "turn off system"
 	    to aviod suspend led on after press power button for
 	    resuming from S4.
	4). Add Cmd for TJ85 CPU and Fan table for TJ85 CPU.
	    TJ85 fan table is follow Thermal Fan table V0.6
 	    Cmd 45 Dat 28. 	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 05/09/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.01 (for UMA Golden)        CPU u-code Version:     |
|   KBC BIOS Version   : V1.01 (for C),                                        |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.01 (FD)   :  2A12(FD)                                          |
+==============================================================================+
BIOS:
        1). Fixed Resume from s3, cardreader(pci-e) will re-detect device.
        2). Fixed sometimes ODD will miss under DTM test.
        3). Fixed CRT Detect for WMI ePresentation.
        4). Fixed DTM test fail for Discrete platform.
        5). Add report Security status and ODD type on WMI function.
        6). Add Japanese keyboard support.(write EEPROM offset [F0h]to 4ah first).
        7). Implement DTS function.			
EC:
        1). Update Fan table to follow thermal control table v04.
        2). Check System LED status during "turn off system"
 	    to aviod suspend led on after press power button for resuming from S4.
        3). Enable DTS function.
						
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 05/07/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V1.00 (for UMA Golden)        CPU u-code Version:     |
|   KBC BIOS Version   : V0.25 (for C),                                        |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V1.00 (FD)   : 7C81 (FD)                                          |
+==============================================================================+
BIOS:
        1). Release for Golden.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 05/04/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.25 (for C)                 CPU u-code Version:     |
|   KBC BIOS Version   : V0.25 (for C),                                        |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V0.25 (FD)   : B39C (FD)                                          |
+==============================================================================+
BIOS:
        1). Update Wire LAN Detect fail for WMI.
        2). Added LCD Monitor Backlight control Function for WMI.
        3). Resume from S4 Issue Encountered Under a Specific Programming
            Sequence of the CK505 Derivative Clock Chip.
EC:
        1). Add Panel backlight on/off event function.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 05/01/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.24 (for C)                 CPU u-code Version:     |
|   KBC BIOS Version   : V0.24 (for C),                                        |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V0.24 (FD)   : 42B8 (FD)                                          |
+==============================================================================+
BIOS:
        1). Solved DTM test fail at USB 2.0.

EC:
        1). Fixed Eurokey and USDkey will send abnormal scancode at DOS mode.
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 04/29/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.23 (for C)                 CPU u-code Version:     |
|   KBC BIOS Version   : V0.23 (for C),                                        |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V0.23 (FD)   : 5BF8 (FD)                                          |
+==============================================================================+
BIOS:
        1). Update LAN cable detect for WMI.
        2). Remove Change and Disable HDD password status under SCU.

EC:
        1). Fixed issue for system entering S4 -> remove AC -> AC LED still on.
        2). Add Cable in/out event function.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 04/24/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.22 (for C)                 CPU u-code Version:     |
|   KBC BIOS Version   : V0.22 (for C),                                        |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V0.22 (FD)   : B061 (FD)                                          |
+==============================================================================+
BIOS:
        1). Add Brightness support Vista.
        2). Fixed Screen flash for a second when exit Saving Change under SCU.
        3). Change Acer Logo background color, change F2 and F12 string color.
        4). Modift WMI Function.
            1. Added get PCI device information
            2. Update LAN connect Event
        5). Fixed "SCU hang in save and exit".
        6). Fixed sometimes hang on post code 94h.
        7). Fixed Save change will reboot under SCU.
EC:
	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 04/17/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.21 (for C)                 CPU u-code Version:     |
|   KBC BIOS Version   : V0.21 (for C)                                         |
|   VGA BIOS(uma)      : Intel 1471                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V0.21 (FD)   : D75A (FD)                                          |
+==============================================================================+
BIOS:
        1). Reduce post time.
        2). Fixed battery utitly test fail.
        3). Fixed T5450 cpu can't enter C3 states.
        4). Solved when resume from s3, Card reader device disappear.
        5). Fixed After flash bios use Crisis Disk, the system DMI string will be clean
        6). Solved Hitachi and Toshiba HDD was late 2~3 at post time.
        7). 17" platform with two HDD can't install OS on Disk-0, only can install on Disk-1.
        8). Implement always Reboot after Save SCU Setting.It Reboot after, change hdd password only under SCU.
        9). Can't boot up in DC mode.
        10).Fixed PC beep can't work.
EC:
	      1). Modified ADPI voltage and throttling time to follow battery parameter.
	      2). Modified Brightness control hotkey.	
	      3). Modified TurnOffKBC behavior for wrong adapter function under system off mode.	
	      4). Modified battery manufacturer name behavior.
	      5). Update KB925/926 source code all v0.21.
	      6). Update Fan table to follow thermal control table v03.
	      7). Modified Fn+S->A function to support store port80 information in system off mode when Fn+S->A is pressed.
	      8). Modified EC_MUTE behavior. 	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 04/11/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.20 (for C)                 CPU u-code Version:     |
|   KBC BIOS Version   : V0.20 (for C)                                         |
|   VGA BIOS(discrete) : ATI Ver009.012.001.025.023754                         |
|   VGA BIOS(uma)      : Intel 1436                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V0.20 (FD)   : B0F7 (FD)                                          |
+==============================================================================+
BIOS:
        1). Remove wake up function for PCIE port 2,3,4.
        2). Improve Power Consumption
        3). Cold boot and S4 resume hang on logo after set hdd password
        4). ICK70 two hdd platform set hdd password can hang on post logo
        5). Enable HPET function on ASL code.
        6). Resume from s4, WLAN device status turn off and can't turn on
        7). Press F12 button on post cause F2 string disppear, when disable F12 boot menu item.
        8). When press F12 key, F12 string glisten .
        9). Int15h AX=9610h Sub-Function 0C, get product name incorrect.
        10).Modify Setup menu <F5> and <F6> key to match acer specification.
        11).Added ATI VBIOS M74/M76 version string at setup menu.
        12).Fixed HD password state incorrect.
        13).After install OS finish, have a "High Definition Audio Controller" show
            exclamation mark in Device Manager.Fail with ATI M74M/M76M platform.
        14).Fixed some new card can't hot plug
        15).UMA system will hang in Enable/Disable PCI Bridge 2448
EC:
	      1). Modify TP enable/disable behavior to fix disable ALPS TP and enter S3
	          then resume from S3, TP cannot be enabled issue.
	      2). Fix BT power still on after resume from S4. (BT was disable before entering S4)
	      3). Fix sometimes EC can't wake up from reset mode after flash
	      4). Modify SPI ROM replace EEPROM function to prevent sometimes K/B
 	          will be locked
	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 04/02/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.19 (for C)/ V0.19T1 (for B)CPU u-code Version:     |
|   KBC BIOS Version   : V0.19 (for C)/ V0.19T1 (for B)                        |
|   VGA BIOS(discrete) : ATI Ver009.012.001.025.023754                         |
|   VGA BIOS(uma)      : Intel 1436                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V0.19 (FD)   : 4FCF (FD)                                           |
|   Checksum V0.19T1(FD)  : 48F1 (FD)                                           |
+==============================================================================+
BIOS:
        1). Resume from s4, bt device always exist
        2). Fixed show 1394 uuid garbage under Int 15
        3). wireless lan type under Int 15
        4). Serianl Number issue under Int 15
        5). Fixed SD, MS card device and HDA lost when resume from s3
        6). Modify Flash map to skip EEPROM and Boot block
        7). Fixed difficulty into Acer recovery mode when pass ALT+F10
        8). Fixed New card can't use.
        9). Fixed "AcerSystemFrom" -> "AcerSystem" string in F Segment
        10).Solved Boot priority tools fail at PXE boot.
        11).
EC:
	      1). Store Lid status in Namespace.	
	      2). Restore WL & BT status after resume from S4
	      3). Modify FastCharge current for cycle count > 100 and cycle
	          count <= 100.
	      4). Modify EAPD behavior.
	      5). Update Wakeup charging current to 0.5A.
	      6). Fix Synaptics TP crazy caused by moving TP during S3,S4 resume.
        7). Enable RTC wakeup after turn on system to keep SB on unless
            SYSBIOS issue cmd to disable RTC wakeup.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 03/20/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.18 (for B)/ V0.18T03 (for C)CPU u-code Version:    |
|   KBC BIOS Version   : V0.18 (for B)/ V0.18T03 (for C)                       |
|   VGA BIOS(discrete) : ATI Ver009.012.001.025.023754                         |
|   VGA BIOS(uma)      : Intel 1436                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum V0.18 (FD)   : D075(FD)                                           |
|   Checksum V0.18T03(FD) : DD8A(FD)                                           |
+==============================================================================+
BIOS:
        1). Solved Remove AC then attach quickly,system hangs up.
        2). Fixed boot and hibernate resume cause hanged, when hdd password Set.
        3). Fixed when press power button during entering S4, system can't enter S4.
        4). Fixed hang on when press [F2] under Acer Logo.
        5). Fixed password character to match Acer spec.
        6). Implement User level to only view under SCU (for meet Acer Spec).
        7). Update SMBIOS Type 0 & 1 filed to match SMBIOS 2.4 Spec.
        8). Fixed Boot Manager Screen.
        9). Fixed when not plug in AC, can flash bios.
        10). Fixed sometimes happen acer logo disppear.
EC:
        1). Modify Battery LLB condition for S3 from 6% to 5%.


+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 03/13/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.17                   CPU u-code Version:           |
|   KBC BIOS Version   : V0.17                                                 |
|   VGA BIOS(discrete) : ATI Ver009.012.001.025.023754                         |
|   VGA BIOS(uma)      : Intel 1436                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : 8EB2(FD)                                              |
+==============================================================================+
BIOS:
        1). Added load default function to clear user and supervisor
            password when short CMOS jump pin (JP3)
        2). Implement CRISIS function to support ODD.
        3). Improve Power Consumption and Modify Boot string.
        4). Fixed "Boot priority garbage" and can't enter setup menu.
        5). Reduce s3.s4 resume time.
        6). Fixed connect TV tuner, system can't entry C3.C4 mode.
	7). Fixed can't execute Synaptics TouchPad utility.
EC:
        1). Remove "resume from S3 after lid is not pressed" function
        2). Enable wrong adapter protection in system off state.
        3). Remove "arcade button can turn on system under DC mode."
        4). Add 65W/90W adapter function.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 03/02/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.16                   CPU u-code Version:           |
|   KBC BIOS Version   : V0.16                                                 |
|   VGA BIOS(discrete) : ATI Ver009.012.001.025.023754                         |
|   VGA BIOS(uma)      : Intel 1436                                            |
|   Flash Utility Ver: FLASHIT 1.1K & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : C8E5(FD)                                              |
+==============================================================================+
BIOS:
        1). Implement CRISIS function to support Floppy and USB-HDD.
        2). Modify Setup menu and boot menu to meet Acer SPEC.
        3). Update Intel VBios(1436).
        4). Implement HDD password function(WD hdd password s3 resume -> fail).
        5). Added load default function when short CMOS jump pin (JP3).
        6). Fixed sometimes Intel 4965 wireless card SVID lost when long run s3.
        7). Implement SuperVisor/User password function.
EC:
        1). Makes system cannot boot from battery less than 5%.
        2). Modify System Battery Icon shows "In Charging" when EC report
	    100% of capacity to Windows.
        3). Modify scancode to fix "no message when wireless card is not exist".

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 02/27/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.15                   CPU u-code Version:           |
|   KBC BIOS Version   : V0.15                                                 |
|   VGA BIOS(discrete) : ATI Ver009.012.001.025.023754                         |
|   VGA BIOS(uma)      : Intel 1410(070225)                                    |
|   Flash Utility Ver: FLASHIT 1.1  & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,C5h,7dh        |
|   Checksum (FD)      : EA2C(FD)       		                       |
+==============================================================================+
BIOS:
        1). Remove Power on display function on Setup menu.
        2). Can't change "fast boot" item under int15.
        3). Lid switch is "Do nothing".WMP is abnormal when reopen LCD cover.
        4). Lid switch is "Do nothing".Play 3D Mark06.Show error message when reopen LCD cover.
EC:
        1).Remove DPST function.
        2).17" Keyboard add Media Key.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 02/12/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.14                   CPU u-code Version:           |
|   KBC BIOS Version   : V0.14                                                 |
|   VGA BIOS(discrete) : ATI Ver009.012.001.025.023754                         |
|   VGA BIOS(uma)      : Intel 1410                                            |
|   Flash Utility Ver: FLASHIT 1.1  & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh        |
|   Checksum (FD)      : C68C(FD)       		                       |
+==============================================================================+
BIOS:
        1). Solved S4 resume can enter SCU at internal keyboard.
        2). Solved F2&F12 strings too difficult to show.
        3). Fixed F2 into BIOS, whole interface show abnormal.
        4). Fixed F2/F12 string will disappear during Reboot.
        5). Added insert wrong password, it will show warning message under post.
EC:
        1).Modify buttons behavior. Power button will not work while
	    lid switch is pressed.
        2).Modify Store/Retrive TP on/off status to support TP will have
	    same status after resume S3/S4/S5.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 02/07/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.13                   CPU u-code Version:           |
|   KBC BIOS Version   : V0.13                                                 |
|   VGA BIOS(discrete) : ATI Ver009.012.001.025.023754                         |
|   VGA BIOS(uma)      : Intel 1410                                            |
|   Flash Utility Ver: FLASHIT 1.1  & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh        |
|   Checksum (FD)      : 15F3(FD)       		                       |
+==============================================================================+
BIOS:
        1). Enable USB device to support wake up from s3 only for usb port0.
        2). If crazy to press keyboard, keyboard will die on setup menu.
        3). Fixed F2 into BIOS, whole interface show abnormal.
        4). Fixed quickly AC Plug-in/out, system hangs up.
        5). Fix change some items. It will cover BIOS basic interface when Exit.
        6). Speaker no sound after S3 resume.
        7). Change HDD boot priority order to First, after load default.

EC:
        1).Modify buttons behavior. WL,Internet,EMail,BT,Arcade,E-Key
	    will not work while lid switch is pressed.
        2).Disable Fan Full On and add Fan Trip table.
	

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 01/31/2007   |
|------------------------------------------------------------------------------|
|   Major Version      : V0.12                   CPU u-code Version:           |
|   KBC BIOS Version   : V0.12                                                 |
|   VGA BIOS(discrete) : ATI Ver009.012.001.025.023754                         |
|   VGA BIOS(uma)      : Intel 1410                                            |
|   Flash Utility Ver: FLASHIT 1.1  & ENEFLASH.EXE 0.12& Insyde WinFlash 3.17  |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh        |
|   Checksum (FD)      : 8F54(FD)       		                       |
+==============================================================================+
BIOS:
        1). modify SCU VGA Memory size to meet ABO SPEC.
        2). Update Intel VBios 1410 for fix 3d mark issue(must UPDATE Vista DRIVER TO 1158).
        3). Fixed Cursor can be seen before Acer big logo.
        4). Correction ccd type,wireless status, asset tag for int 15 function.
        5). Disable USB device Wake up from S3, S4, S5
        6). Speed up POST Time.
        7). Fixed Could not resume from RTC.
        8). Solved S4 to S3 resume cause cold boot.
        9). Add F1 help function in SCU.

EC:
        1). Modify Wrong adapter function to support wrong adapter check when
	    system is off.
	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 01/19/2007   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.10                     CPU u-code Version:           |
|   KBC BIOS Version : V0.10                                                   |
|   VGA BIOS         : BR22694B.BIN                                            |
|   Flash Utility Ver: FLASHIT.EXE  & ENEFLASH.EXE & Insyde WinFlash 3.17      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh        |
|   Checksum (FD)    : 4616(FD)       		                               |
+==============================================================================+
BIOS:
        1). Correction panel type and touch pad type, wireless status.
        2). Fixed if crazy to press keyboard, keyboard will die on setup menu.
        3). Fixed no IRQ on DOS mode and fixed can't execute test utility of modem.
        4). Correction HDD password Status for Acer Spec.
        5). Update TouchPad EEPROM Address (0xEF --> 0xEE).
        6). Correction SCU Total memory error.
        7). Remove SMI of Power button.(Only support press
            [power button] 4s to shutdown in post process)
        8). Patch MAC Value to UUID EEPROM address.
            (Note: After to falsh bios, first boot no patch it.)
        9). Solved S4 to S3 resume cause cold boot.
        10). Modify press ALT+F10 function key.
        11). Implement CCD Type Detect for Int15.
EC:
	1). Add MIR turn on system from S3,S4,S5 function.
	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 01/15/2007   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.09                     CPU u-code Version:           |
|   KBC BIOS Version : V0.09                                                   |
|   VGA BIOS         : BR22694B.BIN                                            |
|   Flash Utility Ver: FLASHIT.EXE  & ENEFLASH.EXE & Insyde WinFlash 3.17      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh        |
|   Checksum (FD)    : 2513(FD)       		                               |
+==============================================================================+
BIOS:
        1). Fixed S4 resume to press key-event problem.
        2). Correction SCU HDD information.
        3). Modify SMBIOS Table.
        4). "Network Boot" function disable, [b57diag] tools can't detect the Lan device.
        5). Add Win Flash function.
        6). Implement CIR/MIR function.
EC:
	1). Modify EC_Mute behavior to avoid abnormal bobo sound.
	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 01/08/2007   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.08                     CPU u-code Version:           |
|   KBC BIOS Version : V0.08                                                   |
|   VGA BIOS         : BR22694B.BIN                                            |
|   Flash Utility Ver: FLASHIT.EXE  & ENEFLASH.EXE & Insyde WinFlash 3.17      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh        |
|   Checksum (FD)    : 9CA4(FD)       		                               |
+==============================================================================+
BIOS:
        1). Correction SCU Boot item.
        2). Add int15 Function.
        3). Solved Acer's D2DRecover function report status error.
        4). Fixed When flash complete, can't shutdown.
        5). Add Win Flash function.

EC:
	1). Enable Wireless LAN when system on.
	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 01/02/2007   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.07                     CPU u-code Version:           |
|   KBC BIOS Version : V0.07                                                   |
|   VGA BIOS         : BR22694B.BIN                                            |
|   Flash Utility Ver: FLASHIT.EXE  & ENEFLASH.EXE & Insyde WinFlash 3.17      |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh        |
|   Checksum (FD)    : A5B9(FD)       		                               |
+==============================================================================+
BIOS:
        1). Added PMC SPI ROM Part.
        2). Fixed "There is a line(grabag) leave in BIOS setup menu when load
            BIOS default setting(select NO) in Information page".
        3). Fixed up Modem SVID and SDID fail.
        4). Fixed "In bios setup menu press F9 to load default settings.
            the screen will shake.
        5). Fixed "17" HDD board can't select boot disk from <JP3> channel 4".

EC:
	1). Modify Fn+F3 scancode to fix Fn+F3 does not work issue.
	2). Modify Hotkey function for Fn-F5.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 12/26/2006   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.06                     CPU u-code Version:           |
|   KBC BIOS Version : V0.06                                                   |
|   VGA BIOS         : BR22694B.BIN                                            |
|   Flash Utility Ver: FLASHIT.EXE  & ENEFLASH.EXE                             |
|   Clock Generator(discrete): 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh     |
|   Clock Generator(UMA)  : 01h,85h,ech,fdh,ffh,f0h,33h,11h,d0h,65h,7dh        |
|   Checksum (FD)    : DAB8(FD)       		                               |
+==============================================================================+
BIOS:
        1). Power On Display function is correction.
        2). Fill All device SVID & SDID.
        3). Add PC beep Function.
        4). Fix up Can't Boot with USB2.0 on USB port3.
        5). Fixed can't display on CRT for Intel VGA.
        6). Modify Clock generate register.
EC:
	1). Fix Power on LED still light in S4.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 12/18/2006   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.05                     CPU u-code Version:           |
|   KBC BIOS Version : V0.05                                                   |
|   VGA BIOS         : BR22694B.BIN                                            |
|   Flash Utility Ver: FLASHIT.EXE  & ENEFLASH.EXE                             |
|   Clock Generator  : 001h, 0FFh, 024h, 02Ch, 02Dh, 0E0h		       |
|   Checksum (FD)   : 5B58(FD)           		                       |
+==============================================================================+
BIOS:
        1). Fix up New Card Hot Plug Fail.
        2). Update Intel VGA BIOS.
        3). Fix Card reader miss SVID & SDID after S4 resume.
        4). Add modem ring up function.
        5). Fix up SD& MMC Card Reader Write Protect Fail after S3 Resume.
        6). Fixed "In Dos mode,press Ctrl+Alt+Del after restart system will shutdown.
        7). If plug in battery, OS can't report battery status immediately.
        8). Fixed can't report cpu thermo for Intel TAT Utility.

EC:
	1). Update Brightness Table -- Panel ID and DAC value
	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 12/11/2006   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.04                     CPU u-code Version:           |
|   KBC BIOS Version : V0.04                                                   |
|   VGA BIOS         : BR22694B.BIN                                            |
|   Flash Utility Ver: FLASHIT.EXE  & ENEFLASH.EXE                             |
|   Clock Generator  : 001h, 0FFh, 024h, 02Ch, 02Dh, 0E0h		       |
|   Checksum (FD)   : 9DE4(FD)           		                       |
+==============================================================================+
BIOS:
        1). Fix up SD/MMC card can't save file in it, and SD card lock still
            can save file.
        2). Fixed s3 resume fail on Discrete platform.
        3). Include SLP2.0 for ACER only.
        4). 1394 GUID READ FROM EEPROM.
        5). Fixed cpu speed can't run min speed.
        6). Modify Acer Quick Boot function.
        7). Take off post image string at boot screen and modify F2 with F12
            function string.

EC:
	1). Reverse BT and WL Button Matrix value to fix Wireless LAN and
	    Bluetooth can't enable/disable by switch button.
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 12/05/2006   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.03                     CPU u-code Version:           |
|   KBC BIOS Version : V0.03                                                   |
|   VGA BIOS         : BR22694B.BIN                                            |
|   Flash Utility Ver: ENEFLASH.EXE                                            |
|   Clock Generator  : 001h, 0FFh, 024h, 02Ch, 02Dh, 0E0h		       |
|   Checksum (FD)   : 2082h(FD)           		                       |
+==============================================================================+
BIOS:
        1). Fixed warm boot will hang on post code "BE".
        2). Modify verbtable when weigh in modem device.
        3). Fixed Can't display on Panel for Intel VGA.
        4). Implement SMBIOS with EEPROM at SCU
        5). Remove internal VBios using Ext.VBios for ATI VGA.

EC:
	1). Switch Battery OVP temperature definition on 6 and 8 Cell battery.

+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 11/29/2006   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.02                     CPU u-code Version:           |
|   KBC BIOS Version : V0.02                                                   |
|   VGA BIOS         : BR22694B.BIN                                            |
|   Flash Utility Ver: ENEFLASH.EXE                                            |
|   Clock Generator  : 001h, 0FFh, 024h, 02Ch, 02Dh, 0E0h		       |
|   Checksum (FD)   : 6BBFh(FD)           		                       |
+==============================================================================+
BIOS:
        1). Fixed CPU can't run High speed.
	2). Fixup Can't detect IEEE 1394 device and xD show "You need to Format".
	3). Implement Save Setup Menu Value.
	4). Implement Realtek Audio verbtable and modem.
	5). Remove Pci-E Port 5 & 6.
	6). Implement Lid Switch function.
	7). Fixed new card can't hot plug.
	8). Fixed s3 can't resume.

EC:
	1). Enable CPU over temp. shtudown function.
	2). Add DVR(Digital Volume Control) function.
	3). Enable battery OVP protection function.
	
+==============================================================================+
| MODEL NO. :  ICL50                               RELEASE DATE : 11/21/2006   |
|------------------------------------------------------------------------------|
|   Major Version    : V0.01                     CPU u-code Version:           |
|   KBC BIOS Version : V0.01                                                   |
|   VGA BIOS         : BR22694A.BIN                                            |
|   Flash Utility Ver: ENEFLASH.EXE                                            |
|   Clock Generator  : 001h, 0FFh, 024h, 02Ch, 02Dh, 0E0h		       |
|   Checksum (FD)   : 46AEh(FD)           		                       |
+==============================================================================+

BIOS:
        1). Update ASL code.
	2). 5787 LAN option ROM include.
	3). Fix 1394 and Ricoh card reader show yellow marker
	4). Add acerint 15 function interface
	5). Modify GPIO setting.
	6). Implement Intel VGA BIOS.
	7). Implement Acer SCU function.

EC:
	1). Wake on Lan function refers to WOL_EN pin.
	2). Add BT,WL,EKey,Email and IE button function.
	3). Disable WatchDog function.
	4). Fan always full on.
	5). Disable Thermal over temperature shutdown
	6). Disable Battery OVP
