+============================================================================+
KAW60 Release Note
+============================================================================+

BIOS CORE Version ................  Phoenix FirstBIOS
CPUs Supported    ................  AMD AM2 2650e (15W)
Chipset		  ................  ATI RS690M
Bridge		  ................  ATI SB600
Video		  ................  ATI RS690M UMA
LAN               ................  Realtek RTL8102EL
KBC		  ................  ENE KB926
CODEC             ................  ALC268
Modem             ................  MDC 1.0
WLAN              ................  Broadcom/Atheros
Clock Generator   ................  ICS951462
BIOS ROM (1MB)    ................  MX25L8005

##############################################################################
#       								     #
#	The "*" mark indicates that file has been modified in this version.  #
#	The "+" mark indicates that file has been added for issue fix.	     #
#	The "-" mark indicates that file has been removed for some reason.   #
#									     #
##############################################################################
+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 09/30/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V1.03                                          |
|           KBC BIOS Version: V1.03 	                                     |
|           Kernel   Version: V1.56 (2008/08/13)                             |
|           EC Firmware Ver.: K4BA103A.ROM (2008/09/30)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029773 (UMA)  		     |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 00h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 2644 h  	   	                             |
|               ROM CHECKSUM: B8C4 h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fixed Vista x64 system with bundled 4G DRAM will hang up after resume from S3.
	02.> Fixed Toshiba HDD Show F1 Error Message when S4 Resume.

<EC BIOS>
 Fixed:
	01.> Disable debug message to slove Run in TP no function issue.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 09/10/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V1.02                                          |
|           KBC BIOS Version: V1.02 	                                     |
|           Kernel   Version: V1.56 (2008/08/13)                             |
|           EC Firmware Ver.: K4BA102A.ROM (2008/09/10)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029773 (UMA)  		     |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 00h  ( Updated )                       |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: F19C h  	   	                             |
|               ROM CHECKSUM: 861C h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fix BTS(V6.2.8) fail items of SB600(CIMX v5.0).
	02.> Fix S3 Stress IO Failed of DTM.
	03.> Fix TTK CPU Can't Boot.
	04.> Disable CLKREQC# controls SRC0(CLK_PCIE_MINI).
	05.> Programming SILEGO SLG84605 ClockGen.
	06.> Correct BIOS Coding of Sleep Type Setting.

<EC BIOS>
 Fixed:
	01.> Fixed FR Keyboard hotkey no function issue.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 09/03/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V1.01                                          |
|           KBC BIOS Version: V1.01 	                                     |
|           Kernel   Version: V1.56 (2008/08/13)                             |
|           EC Firmware Ver.: K4BA101B.ROM (2008/09/03)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029773 (UMA)  		     |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 52E1 h  	   	                             |
|               ROM CHECKSUM: E961 h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fix S3 Black Screen at Debug Code 0x1D.
	02.> Fix S4 Can't Auto Resume.

<EC BIOS>
 Fixed:
	01.> Fix S3 Black Screen.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 08/27/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V1.00                                          |
|           KBC BIOS Version: V1.00 	                                     |
|           Kernel   Version: V1.56 (2008/08/13)                             |
|           EC Firmware Ver.: K4BA100A.ROM (2008/08/27)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029773 (UMA)  		     |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: A4F0 h  	   	                             |
|               ROM CHECKSUM: 39B2 h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	Based on V0.12 BIOS to rename to golden BIOS V1.00.

<EC BIOS>
 Modified:
	Rename from K4BA012A to K4BA100A.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 08/21/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.12                                          |
|           KBC BIOS Version: V0.12 	                                     |
|           Kernel   Version: V1.56 (2008/08/13)                             |
|           EC Firmware Ver.: K4BA012A.ROM (2008/08/21)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029773 (UMA)  		     |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 174B h  	   	                             |
|               ROM CHECKSUM: ACCB h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fixed BTS (V6.2.8) fail items of CPU (AGESA V3.1.9.1).
	02.> Fixed BTS (V6.2.8) fail items of RS690 (CIMX v3.4) and SB600 (CIMX v5.0).
	03.> Removed 2nd Thermal Zoon (Not Support).
	04.> Modified S3 SIO Code Defaulte Behavior:
	     (1) SIO S3 Save Config    ==> Do nothing
	     (2) SIO S3 Restore Config ==> Do nothing

	05.> Modified ASL Code for SBIOS to program Common Clock & ASPM L1.
	06.> Added S3 Debug Code (S3 Restore 0x1D).

<EC BIOS>
 Fixed: 01.> Modified Keyboard matrix to fix CCIC023 UK keyboard have two key
	     no function issue.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 08/14/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.11                                          |
|           KBC BIOS Version: V0.11 	                                     |
|           Kernel   Version: V1.56 (2008/08/13)                             |
|           EC Firmware Ver.: K4BA011A.ROM (2008/08/14)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029773 (UMA)  		     |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 5B4E h  	   	                             |
|               ROM CHECKSUM: EECE h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fixed the system will show bluescreen (error code FE) or garbage
	     after restarting system when doesn't recognize the USB Speaker.
	02.> Removed AC97 Controller ASL Code.
	03.> Modified INT15 to Match String "eMachines" for MP.
	04.> Updated Kernel Default Values From Below Spec :
	     (1) RS690 RPR V3.02 page3-8 3.4.1
	     (2) RS690 RPR V3.02 page3-8 3.4.1.1
	     (3) RS690 RPR V3.02 page3-9 3.5

<EC BIOS>
 Fixed: 01.> Modified wrong adapter protection parameter.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 08/11/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.10                                          |
|           KBC BIOS Version: V0.10 	                                     |
|           Kernel   Version: V1.54 (2008/08/08)                             |
|           EC Firmware Ver.: K4BA010A.ROM (2008/08/11)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029773 (UMA)  		     |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 7D1C h  	   	                             |
|               ROM CHECKSUM: 10C4 h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Added Below Items into INT15 to Match Acer INT15 Spec.
	     WLAN Card :(1) Ralink card.
		  	(2) Atheros n-card.

	     Sub-brand :(1) EMACHINES
		  	(2) PacBel
		  	(3) Gateway

	     Panel type:(1) 1920 x 1080  WUXGA (FHD, 1080P)
		  	(2) 1680 x  945  WXGA+ (HD+,  720P)
		  	(3) 1024 x  600  WSVGA
		  	(4) 1024 x  576  WSVGA
		  	(5) 1366 x  768  WXGA
		  	(6) 1280 x  720  WXGA

	     CCD type  :(1) LiteOn

	02.> Updated Kernel Default Values From Below Spec :
	     (1) RS690 RPR V3.02 page 2-8 2.15
	     (2) RS690 RPR V3.02 page 7-8 7.7.1
	     (3) RS690 RPR V3.02 page 7-10 7.7.5

<EC BIOS>
 Fixed: 
	01.> Rename from K4BA009A to K4BA010A.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 08/07/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.09                                          |
|           KBC BIOS Version: V0.09 	                                     |
|           EC Firmware Ver.: K4BA009A.ROM (2008/08/07)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029773 (UMA)  		     |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 47BB h  	   	                             |
|               ROM CHECKSUM: DBBC h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fixed Press Power Button Caused White Screen Issue when BIOS POST.
	02.> Fixed Boot Hang Up at Debug code 0x54 when Press F2 Key
             Continuos on Text Mode.
	03.> Tri-stating the processor's HT link when LDTSTOP_L is asserted.
	04.> Correct BTS fail item of south bridge.
	05.> Modified Setup Menu to hide below items :
	     Menu : Advance Menu
		    Miser   Menu
	     Item : Floppy A (in Main Menu)

<EC BIOS>
 Fixed: 
	01.> Fix [BCIC100] Battery over temp. function trigger point can't meet spec issue.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 08/04/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.08                                          |
|           KBC BIOS Version: V0.08 	                                     |
|           EC Firmware Ver.: K4BA008A.ROM (2008/08/04)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029773 (UMA, BR29773.bin)      |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 548E h  	   	                             |
|               ROM CHECKSUM: EA02 h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Speed Up Boot Time.
	02.> Fix System Momory Size Not Correct when Attached 4GB Memory.
	03.> Modified INT15 String (eMachine --> eMachines) for Meet eMachine Spec.
	04.> Add Debug Code for Battery Plug In/Out Event.
	05.> Updated Formal VBIOS (BR29773.bin) to Solve the SKU1 (AUO Panel)
             Blink White Flicker Issue.
	06.> Correct BTS fail items.
	07.> Correct SATA Driving Strength.
	08.> Fix SMBIOS Type4 Fail Item of DTM Test (Update Kernel)

<EC BIOS>
 Fixed: 
	01.> Fix after Crisis, system won't restart issue.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 07/31/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.07                                          |
|           KBC BIOS Version: V0.07 	                                     |
|           EC Firmware Ver.: K4BA007A.ROM (2008/07/31)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029720 (UMA, BR29720.bin)      |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 9D33 h  	   	                             |
|               ROM CHECKSUM: 30A7 h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fix Boot Hang Up when Press F2 Key Continuos on Text Mode.
	02.> Fix Legacy USB Keyboard Can't be Used, Must Press Internal Keyboard Any Key First.
	03.> Fix LAN Loop Back Test Hang.
	04.> Fix DMI Type0 String Not Correct.
	05.> Modify DMI Type8 for Meet Platform Spec.
	06.> Modify GUI of S4 Resume Logo.
	07.> Modified INT15 String for Meet eMachine Spec.

<EC BIOS>
 Fixed: 
	01.> Fix <BCIC080> Disable Touch Pad by Fn+F7, touch pad still have function.
	02.> Fix <BCIC015> Touch pad will have no function at first click or move.

 Modified:
	01.> Fine tune fan table.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 07/29/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.06                                          |
|           KBC BIOS Version: V0.06 	                                     |
|           EC Firmware Ver.: K4BA006A.ROM (2008/07/29)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.0000000 (UMA)		     |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: FE33 h  	   	                             |
|               ROM CHECKSUM: 9243 h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Change Throttling Function to Do P-State.
	02.> Correct CPU BTS fail item.
	03.> Solved S3 black screen & 3D Mark hang up in DC mode.
	04.> Fix can't enter S3 via LID after S3 resume

<EC BIOS>
 Modified:
	1.> Modified Battery OTP throttling temperature from 60 to 68.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 07/24/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.05                                          |
|           KBC BIOS Version: V0.05 	                                     |
|           EC Firmware Ver.: K4BA005A.ROM (2008/07/24)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029455 (UMA)                   |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 37h (changed by SYS BIOS 06.)          |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 1DCC h  	   	                             |
|               ROM CHECKSUM: B1DC h  	   	                             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fix Azalia Verb Table Lose after S3 Resume.
	02.> Enabled ASPM Function.
             Removed Alink and GPP ASPM override (for AMD suggestion).
	03.> Fix SLP2.0 Fail.
        04.> Set Mobile Type of FACP Table to Fix Hibernate Item Disappears.
        05.> There have garbage or system abnormal after S3 resume when HDD
             password has been enabled.
        06.> PCIE Spread Spectrum Enabled for EMI Requested.
             * SRC= 100MHz, Spread= -0.25%, SRC OverClock= 0%

<EC BIOS>
 Fixed: 
	1.> Fix Fn+home/pg up/pg dn/end have no function issue.
	2.> Fix backlight can be turn on by pressing USB Keyboard issue.
	3.> Fix system can boot up with RSOC<=5% under battery only mode issue.
	4.> Fix enable Num lock, special letter output is different from
            the real print

 Modified:
	1.> Modified fan table for Thermal team.

 Add function:
	1.> Add crisis function.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 07/21/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.04                                          |
|           KBC BIOS Version: V0.04 	                                     |
|           EC Firmware Ver.: K4BA004A (2008/07/21)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029455 (UMA)                   |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 17h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: F113h  	   	                             |
|               ROM CHECKSUM: 8523h		             	             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fix Camera Detected Fail of ACER INT15 Function.
	02.> Fix Fan Full Speed
	03.> Fix BIOS Menu VRAM Size Can Be Control of User Authority
        04.> Add Debug Feature

<EC BIOS>
 Fixed:
	1.> Fix fan always on with full speed.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 07/16/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.03                                          |
|           KBC BIOS Version: V0.03 	                                     |
|           EC Firmware Ver.: K4BA003A (2008/07/16)	                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029455 (UMA)                   |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 17h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: 3ED8h  	   	                             |
|               ROM CHECKSUM: D3C7h		             	             |
|                                                                            |
+============================================================================+
<SYS BIOS>
	01.> Fix PXE LAN Boot Item Lose in BIOS Setup Menu after Execution
             BS Utility to Change BIOS Boot Sequence.
	02.> Fix CMOS Error Message when First Boot after Flash BIOS
	03.> Fix F10 Boot Menu String will show in Setup Menu
	04.> Fix OS Hang Up when Plug In USB Devices after S3 Resume
	05.> Fix Vista OS Brightness Controll Fail
        06.> Modify The Rule of ABO UMA Share Memory Size
	07.> Enable SB Throttling Function and CPU C2/C3 State
	08.> Modify GUI Message for Meet KAW60 BIOS Spec V0.02
	09.> Modified Setup Menu Items Description for Meet KAW60 BIOS Spec V0.02
	10.> Added Power On Display Function
	11.> Set User Password Dependent Supervisor Password for ACER Spec

<EC BIOS>
 Fixed:
	1.> Fix EC send throttling SCI when resume from S3 every time.
	2.> Fix no sound in DOS mode.
	3.> Fix wireless switch no function issue.
	4.>

 Modified:
	1.> Remove Fn+F1/F2/F3 hot key function from KBC code for this new KB layout.
	2.> Modify name space for BIOS.

 Added Function:
	1.> Add SPI protection.

+============================================================================+
| MODEL NO. : KAW60                              RELEASE DATE : 07/12/2008   |
|----------------------------------------------------------------------------|
|           SYS BIOS Version: V0.02                                          |
|           KBC BIOS Version: V0.02  	                                     |
|                                                                            |
|           VGA BIOS Version: 010.055.000.049.029455 (UMA)                   |
|                                                                            |
|        VGA Clock Frequency:                                                |
|                      UMA:300MHz M52:392MHz M56:475MHz M62:425MHz M66:460MHz|
|                                                                            |
|       VRAM Clock Frequency:                                                |
|                      UMA:xxxMHz M52:375MHz M56:375MHz M62:375MHz M66:375MHz|
|                                                                            |
|         Support Panel Type: EDID                                           |
|                                                                            |
|    Clock Generator Setting: Byte0 : 17h                                    |
|                             Byte1 : 7Dh                                    |
|                             Byte2 : 10h                                    |
|                             Byte3 : 65h                                    |
|                             Byte4 : 01h                                    |
|                                                                            |
|     DOS Phlash Utility Ver: Version 1.6.7.0                                |
| Windows Phlash Utility Ver: Version 0.01                                   |
|                                                                            |
|               WPH CHECKSUM: E4CAh     	                             |
|               ROM CHECKSUM: 7614h             	                     |
|                                                                            |
+============================================================================+
<SYS BIOS>
First Formal Release

<EC BIOS>
 Fixed:
	1.> Fix wireless switch no function issue.
	2.> Fix wireless LED behavior abnormal issue.
	3.> Fix battery device name dection issue.
	4.> Fix can't resume from S4 by Pwrtest.

 Modified:
	1.> Modify Power button status.
	2.> Modify to prevent show Battery Charge 0% when Battery Charge to 100% or >95%.
	3.> Add scan code of Fn for production.
	4.> Modify battery TS Pin parameter.
	5.> Modify panel brightness table
