
                           README FILE
                         January 22, 1997
              Iomega Adapter Support under Windows NT
     
     Contents
     
     Section # Topic
           1   Installing Adapter Support under Windows NT
           2   Driver Installation from the Iomega Install
               Diskette
                    Under version 4.0
                    Under version 3.51
           3   Installation for Native NT Adapter Drivers
                    Under version 4.0
                    Under version 3.51


     _________________________________________________________
     Section 1
     Installing Adapter Support under Windows NT

     If you are installing a new adapter, you MUST install the
     adapter driver on your system BEFORE you can install ToolsNT
     software to support your Iomega drive.  If you are
     installing a Jaz jet PCI adapter, Jaz Traveller, or parallel
     port Zip drive, install the necessary Iomega driver from the
     Windows NT Install diskette that came with the adapter or
     drive (see Section 2 for instructions).  For other Iomega
     adapters, install the native NT driver support included with
     Windows NT (see Section 3 for instructions).  If you are
     using a non-Iomega SCSI adapter, refer to your Windows NT
     documentation for instructions on installing a SCSI adapter
     or refer to the documentation that came with the adapter.


     _________________________________________________________
     Section 2
     Driver Installation from the Iomega Install Diskette

     The Iomega Install diskette for Windows NT that ships with
     your Iomega drive or adapter includes software drivers for:

         Iomega parallel port products (including Jaz Traveller
          and the parallel port Zip drive) 

         Jaz jet PCI (PC/Mac model)
     
     You can install either of these drivers using the following
     procedures.


     ______________________________
     Section 2.1
     Iomega Driver Installation under Windows NT 4.0

      1.  Click Start, point to Settings, then click Control
          Panel.

      2.  Double click "SCSI Adapters."

      3.  Select the "Drivers" tab and click the "Add" button.

      4.  Click "Have Disk" and insert the Iomega Install
          diskette for Windows NT into the computer's floppy
          drive.

      5.  Click "Browse" and select the drive letter for the
          floppy drive.

      6.  Select the folder for the adapter you are installing
          and click "Open," then click "OK."

      7.  When the list of Iomega adapters appears, highlight the
          adapter you are using and click "Next" to continue.

      8.  Click "OK" for Windows NT to install the necessary
          adapter drivers on your system.

      9.  Click "OK" to exit.  Note that you need to reboot your
          system for the new drivers to take effect.


     ______________________________
     Section 2.2
     Iomega Driver Installation under Windows NT 3.51

      1.  From the Windows NT Main icon, double-click on the
          Windows NT Setup icon.

      2.  From the Setup window, choose the Options pull-down
          menu, select "Add/Remove SCSI adapter," then click
          "Add."

      3.  Scroll down the adapter list box and click on "Other."

      4.  Insert the Iomega Install diskette for Windows NT into
          the computer's floppy drive.

      5.  Select the drive letter for the floppy drive and the
          folder for the adapter you are installing, then click
          "OK."
     
      6.  When the list of Iomega adapters appears, highlight the
          adapter you are using and click "OK."

      7.  Click "Install."  Windows NT will automatically copy
          the driver files and add the driver to the list of
          adapters found by the operating system.

      8.  Reboot your computer to configure the driver for your
          system.


     _________________________________________________________
     Section 3
     Installation for Native NT Adapter Drivers

     Windows NT includes native driver support for the following
     Iomega adapters:

         Jaz jet ISA

         Jaz jet (PC-only model)

         Zip zoom

         PC1600


     ______________________________
     Section 3.1
     Native Driver Installation under Windows NT 4.0

      1.  Click Start, point to Settings, then click Control
          Panel.

      2.  Double click "SCSI Adapters."

      3.  Select the "Drivers" tab and click the "Add" button.

      4.  Select "Adaptec" from the list of manufacturers.

      5.  When the list of Adaptec SCSI Adapters displays, select
          the driver needed for your adapter:

              for Jaz jet ISA, Zip zoom, or PC1600,
               click on "Adaptec AHA-152x/AHA-1510 SCSI Host
               Adapter"

              for Jaz jet (PC-only model),
               click on "Adaptec AHA-294x/AHA-394x or AIC 78xx
               PCI SCSI Controller"

      6.  Click "Next" to continue, then click "OK" for Windows NT
          to install the necessary adapter drivers on your
          system.

      7.  Click "OK" to exit.  Note that you need to reboot your
          system for the new drivers to take effect.



     ______________________________
     Section 3.2
     Native Driver Installation under Windows NT 3.51

      1.  From the Windows NT Main icon, double-click on the
          Windows NT Setup icon.

      2.  From the Setup window, choose the Options pull-down
          menu, select "Add/Remove SCSI adapter", then click Add.

      3.  Scroll down the adapter list box and click on the
          driver needed for your adapter:

              for Jaz jet ISA, Zip zoom, or PC1600,
               click on "Adaptec 151x/152/AIC 6260/6360"

              for Jaz jet (PC-only model),
               click on "Adaptec 294x/AIC 78xx (PCI)"

      4.  Select "Install," and then choose "Current" in the next
          dialogue box.  The Adaptec driver for your adapter
          should appear in the window listing adapters found by
          Windows NT.

      5.  Reboot your computer to configure the driver for your
          system.
