README.TXT for Intel EtherExpress 10/100 Series Driver Installation
===================================================================

To install the drivers and utilities for the Intel EtherExpress 10/100 series Network Adapter,
follow these instructions:

1.  If you are in Windows 95, open a DOS session by clicking on the MS-DOS
    Prompt icon.

2.  At the DOS prompt, type "INTEL100 -d -o c:\" and press ENTER.  This will
    extract the drivers to the "A" directory on your C drive.

3.  In Windows 95, open My Computer, Select the C: drive and open the "A"
    folder.

4.  From this folder open the Disk1 folder.  Locate and double click on the
    SETUP icon.

5.  Follow the instructions on the screen. 

6.  After the installation has completed successfully, you may remove the
    "A" folder from your C: drive by opening "My Computer", Opening the
    "C:" drive and selecting the "A" folder.  Once selected, press the DEL
    key on your keyboard.  Answer "YES" to remove this folder from your hard
    drive.

-END-
