=======================================================================
Viper V330 Series                                            README.ENG
=======================================================================

Installation Notes
------------------

CD Installation
---------------

The Windows 95 drivers contained on this CD-ROM can be installed directly
from the CD-ROM. First you must have Windows 95 installed with the Standard
VGA driver (640x480x16) before you install the Diamond Viper V330 Series
Windows 95 drivers.  If you are running a different graphics mode please
re-configure for Standard VGA.

After rebooting in VGA mode run the START program from the CD's root
directory: X:\start.exe (Where X is the drive letter of your CD-ROM drive).
Follow the instructions to install the Windows 95 drivers and at the end you
will be prompted to reboot your system.


Manual Installation Instructions
--------------------------------
1.  Once Windows 95 restarts you will want to click the "Start" button, then
    choose "Run...".
 
2.  Now insert the Diamond CD into the your CD-ROM drive and within the "Run"
    dialog box type the following: "x:\WIN95\INSTALL" where x is the 
    corresponding letter of the CD-ROM drive.

       	The following command line switches can be used with INSTALL:

                /f                      This forces a Full installation
                                        (Diamond Viper V330 Series 
					Windows 95 Display Driver and
                                        InControl Tools 95).

                /m                      This forces a Minimal installation
                                        (Diamond Viper V330 Series 
					Windows 95 Display Driver only).

                /d"drive:\path"         This installs InControl Tools 95 into
                                        drive:\path. Note that the quotes, 
                                        drive letter and path are required.
                                        In addition, either the /f or /m
                                        switch must be used in conjunction
                                        with this selection.

                /r                      This forces a system reboot after
                                        installation.  Note that either the /f
                                        or /m switch must be used in
                                        conjunction with this selection.

                /nr                     This prevents a system reboot after
                                        installation.  Note that either the /f
                                        or /m switch must be used in
                                        conjunction with this selection.

                uninstall               This will completely uninstall the
                                        Diamond Viper V330 Windows 95
					Display Driver and InControl Tools 95.
 
3.  Once the Diamond Setup Wizard dialog box appears you will be able to
    review the Readme file or continue on with the installation by selecting
    "Next".
 
4.  The Setup Wizard will now check for Diamond components installed in your
    computer.  Click "Next" to proceed.
 
5.  A dialog box will appear containing the path where InControl Tools 95 will
    be installed.  The default path is:

        "C:\Program Files\Diamond"

    Select "Next" or change the path as necessary.

6.  The next dialog box selects the installation type.  There are three
    installation types: Minimal, Full and Custom.  They are defined as 
    follows:

                Minimal:        This will install only the Diamond Viper V330
                                Series Display Driver.

                Full:           This will install both the Diamond Viper V330 
                                Series Display Driver and InControl 
				Tools 95.

                Custom:         This will allow installation of either the
                                Diamond Viper V330 Series Display
                                Driver or InControl Tools 95.  At the minimum,
                                the Diamond Viper V330 Series 
                                Display Driver must be installed during a
                                first-time installation.

7.  If "Custom" was selected in step 15, a dialog box will appear allowing
    the selection of various items.  Select the items to be installed by 
    clicking on them with the left mouse button.  When finished, click "Next"
    to continue.

8.  At the "Select Files to be copied" dialog box, click "Next" to begin the
    file copying process.
 
9.  After the files have been copied you will want to click "Finish" in order
    to complete the installation.
 
10. Windows 95 will ask that the computer be restarted.  Click on "Yes" to
    restart the computer.
 
11. Once Windows 95 restarts, you will have successfully installed the 
    software for your Diamond Viper V330 Series.  The InControl
    Tools 95 Wizard will then guide you the rest of the way.  Thank you for
    choosing Diamond!


All product names listed are trademarks or copyrights of their
respective owners.

=======================================================================
Diamond Multimedia Systems, Inc.       (c) 1993-97, All Rights Reserved
=======================================================================
