                        3Com (R) Corporation
                    EtherDisk (R) Diskette for the
      3C90X Fast EtherLink XL/EtherLink XL Bus Master NIC Family
                  Banyan VINES Installation Notes


Banyan VINES Client Installations
---------------------------------
To install VINES 6.0 software on a DOS NDIS workstation, follow these
instructions.  DOS must be installed on the target workstation C: drive or
you must have a bootable DOS floppy.

1.  Use the DOS MD command to create a subdirectory called \VINES.

2.  Copy the contents of the VINES LAN S/W (DOS) Install diskette into
    the \VINES subdirectory.

3.  Copy the contents of the NDIS subdirectory on the VINES LAN S/W (DOS)
    2 of 2 diskette into the \VINES subdirectory.

4.  Copy the EL90X.DOS and the PROTOCOL.INI fragment from the NDIS2\DOS
    subdirectory of EtherDisk 1 diskette to the \VINES subdirectory on
    your system.

5.  Edit the PROTOCOL.INI file to read as follows:

    [PROTOCOL MANAGER]
     DRIVERNAME = PROTMAN$

    [VINES_XIF]
     DRIVERNAME = NDISBAN$
     BINDINGS = EL90X

    [EL90X]
     DRIVERNAME = EL90X$

6.  Insert the following lines in the AUTOEXEC.BAT file:

    CD \VINES
    BAN

    BAN loads the NDISBAN drivers.


Banyan VINES Server Installation
--------------------------------

Banyan provides a VINES server driver with the current version of VINES.
Consult the Banyan documentation for installation instructions.

                 (%VER BANYAN.TXT - Banyan VINES v1.0g)


