                        3Com (R) Corporation
                   EtherDisk (R) Diskette for the
      3C90X Fast EtherLink XL/EtherLink XL Bus Master NIC Family
                 MS LAN Manager Installation Notes


Microsoft LAN Manager Versions 2.0, 2.1, and 2.2
------------------------------------------------
The EtherDisk 1 diskette contains a subdirectory structure and files that
make it an OEM import disk for the LAN Manager installer.  Use the import
function of the LAN Manager installer to capture the NDIS driver from the 
EtherDisk diskette.  Be sure to save the new configuration before exiting 
the installer.


DOS Installation with LAN Manager 2.2
-------------------------------------
The following describes the procedure for importing the driver during 
installation of LAN Manager 2.2 for DOS.

1.  Begin the MS-DOS LAN Manager installation by inserting the LAN Manager
    MS-DOS Setup diskette and typing: 
    
    A:SETUP

2.  When the window is displayed showing available network NIC drivers,
    choose: Select Other Driver         (Alt-D)

3.  When prompted to insert your network driver diskette, insert the
    EtherDisk 1 diskette.

4.  After the driver is imported from the EtherDisk 1 diskette, a box 
    appears showing the driver.  Select the Fast EtherLink XL/
    EtherLink XL Bus Master Family driver.

5.  To continue with the remainder of the installation, select a protocol 
    to use with the Fast EtherLink XL/EtherLink XL Bus Master Family driver.
    Continue with the remaining installation steps for Lan Manager.

    
                 (%VER LANMAN.TXT - MS LAN Manager v1.0d)


