Installation Instructions for Yamaha DS-XG sound drivers
--------------------------------------------------------

 1.  From Windows 95 Desktop, click the Start Button.

 2.  Next, click on Settings.

 3.  Click on Control Panel.  A Window will appear.

 4.  Doubleclick on the System icon.  A Window Will appear.

 5.  Select the device manager tab.

 6.  If you see "YAMAHA DS-XG Devices" listed then the drivers are
     installed.

 7.  If you do not see "YAMAHA DS-XG Devices" listed, then doubleclick
     on "Other devices" in the list.

 8.  Select the "PCI Multimedia Audio Device" item.

 9.  Click the "Remove" Button.  When prompted if it is OK to remove
     the device, click OK.

10.  Next, click the "Refresh" button.  Windows will redetect the 
     PCI MultiMedia Audio Device and prompt for the location of the
     drivers.

11.  Click the Next button.  Windows will search for drivers.  If they
     cannot be found, a dialog box will appear.

12.  Click the "Other Locations..." button.

13.  Insert the Product Recovery CD-ROM into the CDROM drive.  If the
     InstallIt Now! program appears, click it's Exit button.

14.  The Select Other Location dialog box will appear.
     Type "Q:\DRIVERS\AUDIO\YAMAHA.XG" into the Location field
     and press ENTER.  The drivers will be installed.

During the driver installation you may be prompted for the location of
certain files.  Type "Q:\DRIVERS\AUDIO\YAMAHA.XG" when prompted.

If the installation prompts that a file being copied is older than the
current version, keep the newer file...Answer "Yes".

Installation Instructions for Yamaha DS-XG sound utilities
----------------------------------------------------------

1.  From Windows 95 Desktop, click the Start button.

2.  Click on "Run".

3.  Insert the Product Recovery CD.  If InstallIt NOW! appears, click
    the exit button.

3.  In the Run dialog box, type:
    "Q:\DRIVERS\AUDIO\YAMAHA.XG\DISK1\SETUP.EXE" and press ENTER.

4.  Follow the on-screen instructions.

-END-
