6x86 Configuration 3.0 - Documentation

Installation : run " setup.exe " from the archive, and follow the instructions.

Under Windows 95 only

"6x86cfg.exe" will be placed in your "autoexec.bat" startup file, in order to configure your CPU for DOS sessions. Edit the autoexec.bat file and add the switches you want in the following.

-FF		Sets the fast framebuffer on
-WA		Sets the Write Allocate option on
-CPUID		Enables the CPUID instruction (makes Windows 95 detect the 6x86 as a Pentium)
-SP		Enables the suspend on HLT option (Power saving)
-DTE		Caches the Directory Table Entries
-NL		Negates #LOCK pin
-DF		Sets the Data Forwarding option on

To deactivate an option, add "N" before the normal switch like this :
to enable : -WA
to disable : -NWA
(note : Activating an option increases performance or functionality)

Windows NT 4.0 and Windows 95
Command line switches

-load : The program will add an icon to the taskbar, giving access to 6x86 Configuration, and configures the processor.

-noicon : When used in conjunction with -load, your processor is configured, but the icon doesn't appear.

To register

If you're happy with this shareware, you may want to register, because this version is limited to a 30 days evaluation.
Go to the Web Page, http://www.chez.com/6x86config/ you will find the instructions there. The registration fee is $20.

You'll get
-The key corresponding to your registration.
-Full technical support
-Free updates

Olivier Gilloire
18 rue de Saint-Blandin
77580 GUERARD
France

Email : 6x86config@chez.com
Web : http://www.chez.com/6x86config/