Note:The behavior of BIOS update is changed!!
1) Before BIOS v1.34,   system will auto restart again when finish update BIOS.
2) After BIOS v1.40,  system will NOT auto restart when finish update BIOS.  System will shut down after update BIOS.  User need to press power button to reboot system.
3) Update BIOS procedure no change, only the last behavior changed.


[SOP]
1. DOS flash: Please kindly unzip the <ICL50144A.zip> under windows mode and do system reboot to boot to pure Dos mode. Then, clcik "IF50.bat" batch file to update bios under pure Dos mode.
2. Windows flash: Please kindly unzip <ICL50144_Winflash.zip> under windows mode and click "ICL50144.exe" to update bios.
